Embedded Control Game Report

Michael Stark & David Melecio-Vázquez

Section 4, Side A (TA: Xuemei Gao)

Due: 8 October 2010

Table of Contents

[I. Introduction and Statement of Purpose 3](#_Toc274132985)

[II. System Development 4](#_Toc274132986)

[a. Hardware Details 4](#_Toc274132987)

[b. Software Details 9](#_Toc274132988)

[III. Results and Conclusions 10](#_Toc274132989)

[IV. References 11](#_Toc274132990)

[V. Appendices 12](#_Toc274132991)

[a. C code 12](#_Toc274132992)

[b. Hardware schematic 20](#_Toc274132993)

[c. Participation Summary 21](#_Toc274132994)

1. Introduction and Statement of Purpose
2. System Development
   1. Hardware Details

Note: please refer to Appendix B, Hardware Schematic, to see where each component was included in the wiring.

**74F365A Buffer Chip**




Figure 2a-1 - 74F365A Buffer Chip

The Buffer chip is composed of a series of 6 inputs and 6 outputs, each of which is connected with a logical buffer gate.  Outputs such as LEDs and the Buzzer were connected to the microcontroller through the buffer in order to isolate the outputs and protect the components from having current flow across them in the incorrect direction.

**Light Emitting Diode (LED)**

https://lh3.googleusercontent.com/8sGi0q_2c7M5F0q6mjeJS9VCJHh_c6PZaBSsFbvxZiuAmyR36XtULayn9cz60s1cvHS9NAUasVjhnp3g35FUJk8-MlReP2FwFKlRaMrhzLKNd2rGKQ

Figure 2a-2 - LED

A diode is similar to a buffer, in that it only allows current to flow one way through the device.  The LED, however, gives off light when current is flowing in the correct direction.  These LEDs have various shadings on their glass casing, resulting in different colored lights being emitted.  LEDs were used in the hardware as outputs for the User.

**Bi LED**




Figure 2a-3 - Bi LED

The Bi LED component is a simple circuit with two LEDs wired perpendicularly to each other.  When current flows in one direction across the Bi LED, one of the colored LEDs is lit - when current flows in the opposite direction, the other colored LED is lit.  The BiLED was used as an output to the User to indicate various states of the game (e.g. ready to accept input, incorrect input given, etc.).

**Resistor**

https://lh6.googleusercontent.com/URtQ7hrRH-ZcndER7vW8Bg1UtzWXmmTWRVF6JTG4t5PmAkg8hkyfYISBv448RU99gJfMatEyJU-2dAurCi_NvEB4nsu4MTO5ECiyf_Bh5A5a0Nzx6Q

Figure 2a-4 - Resistor

Resistors provide electrical resistance on a circuit.  They are used to absorb some voltage, so that various other components are not overloaded/short circuited by large power surges.  Resistors were used between power and the LEDs, between power and the push buttons, and between power and the potentiometer.

**Potentiometer**

https://lh6.googleusercontent.com/KIlaIPhyH8zuqgYOeh1hU3N8-qY3UhMwowsc-6Ckgx1thYzOkTYWGB2qFKh2TzRgSs_R7GYqrucKzGMVE3cuVRU6DinmB3UW1E_W5MNpxLIIpxFrGA

Figure 2a-5 - Potentiometer

Potentiometers are analog input devices.  By sliding a contact along a resistant surface, a variable amount of voltage is ready along the input wire.  This was used in the game to vary the speed at which LEDs were lit (a larger voltage input resulted in a larger wait time).

**Push Button**




Figure 2a-6 - Push Button

Push Buttons are simple input devices.  When not pressed, an open circuit exists between power and the microcontroller, and a logical high (1) is read.  When pressed a closed circuit is created from power to ground, resulting in a logical low (0) being read in the microcontroller.  Push Buttons were used by the User to indicate which LED was lit, as well as restarting the game.

**Slide Switch**





Figure 2a-7 - Slide Switch Schematic (left) and physical appearance (right)

A slide switch operates similarly to a Push Button, except that the Slide Switch stays in one of two states without the User having to continually press.  Just like the Push Button, in the On position, a closed circuit is formed between power and ground, and a logical low (0) is read on the microcontroller.  In the Off position, an open circuit is formed, and a logical high (1) is read on the microcontroller.  The Slide Switch was used in initial versions of the game to control when the game was played, and to restart the game.

**Buzzer**

https://lh3.googleusercontent.com/sRkbBWqq_aR5E84IBBQ4OkRVQuk4d5-vXGwaaeKQ4DrBp45Yn7PV6ZEZxtn7qirrqAz1bkOnI0KnHovyRH8_0M9EO2qlz7pKdTxBZJH7iB9dCvtobA

Figure 2a-8 - Buzzer

The Buzzer makes a loud buzzing sound when current flows across it.  The Buzzer was used as an output to indicate to the User that incorrect input was given.

* 1. Software Details

1. Results and Conclusions
2. References
3. Appendices
   1. C code

Following is a copy of our file lab2.c.

/\*  
\* Names: Michael Stark + David Melecio-Vázquez  
\* Section: 4 A  
\* Date: 14 September 2010  
\* File name: lab2.c  
\* Description: Play a game of LITEC Memory with the user.  
\*/  
  
#include <c8051\_SDCC.h>// include files. This file is available online  
#include <stdio.h>  
#include <stdlib.h>  
  
//-----------------------------------------------------------------------------  
// Function Prototypes  
//-----------------------------------------------------------------------------  
  
// Initialization Functions  
void Port\_Init(void);      // Initialize ports for input and output  
void Timer\_Init(void);     // Initialize Timer 0   
void ADC\_Init(void);       // Initialize A/D Conversion  
unsigned char Read\_Port\_1(void);       // Performs A/D Conversion  
void Interrupt\_Init(void); // Initialize interrupts  
void Timer0\_ISR(void) interrupt 1; // Called at Timer0 overflow  
  
// Game Functions  
void play\_game(void); // Plays the LITEC Memory game.  
int CalculateMaxCounts(unsigned char x); // Converts the port 1 result into a number of  
                                         // overflows to wait for.  
unsigned char light\_LED(unsigned char LED\_to\_light, short on\_time, short off\_time);

// Light the designated LED for on\_time, then wait for off\_time

unsigned char ReadPushbuttons(); // Wait for a pushbutton event, and return which one was  
                                 // pressed  
unsigned char unique\_random(unsigned char last\_state); // Generates a random number  
                                                       // different from the last one  
unsigned char random(unsigned char N); // Generates a random number between 0 and N-1   
void light\_green(void); // Light BiLED green  
void light\_red(void); // Light BiLED red  
int CheckPushButton1(void); // function which checks push button 1  
int CheckPushButton2(void); // function which checks push button 2  
int CheckPushButton3(void); // function which checks push button 3  
int CheckPushButton4(void); // function which checks push button 4  
char\* newline(); // Helper function, used when printing (returns "\r\n")  
  
//-----------------------------------------------------------------------------  
// Global Variables  
//-----------------------------------------------------------------------------  
  
// Pushbuttons (Inputs)  
sbit at 0xA0 PB3; // Push button 3  
                  // Associated with Port 2, Pin 0 (second from left, red PB)  
sbit at 0xA1 PB4; // Push button 4  
                  // Associated with Port 2, Pin 1 (far left, black PB)  
sbit at 0xA2 PB1; // Push button 1  
                  // Associated with Port 2, Pin 2 (far right, red PB)  
sbit at 0xA3 PB2; // Push button 2  
                  // Associated with Port 2, Pin 3 (second from right, black PB)  
  
// LEDs and Buzzer (Outputs)  
sbit at 0xB2 LED2; // LED2, associated with Port 3, Pin 2  
sbit at 0xB3 BILED0; // BILED0, associated with Port 3 Pin 3  
sbit at 0xB4 BILED1; // BILED1, associated with Port 3 Pin 4  
sbit at 0xB5 LED1; // LED1, associated with Port 3 Pin 5  
sbit at 0xB6 LED0; // LED0, associated with Port 3 Pin 6  
sbit at 0xB7 BUZZER; // Buzzer, associated with Port 3 Pin 7  
  
unsigned int Counts = 0;  
  
  
//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  
void main(void) {  
 Sys\_Init();      // System Initialization  
 Port\_Init();     // Initialize ports 2 and 3   
 Interrupt\_Init();  
 Timer\_Init();    // Initialize Timer 0   
 ADC\_Init();      // Initialize A/D Conversion  
 putchar(' ');    // The quote fonts may not copy correctly into SiLabs IDE  
 putchar('\r');  
  
 // Enable Timer 0  
 TR0 = 1;  
  
 while (!CheckPushButton4()); // Wait for the Start Game button to be pushed  
  
 while (1) {  
   play\_game();  
 }  
}  
  
//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  
void Port\_Init(void) {  
 // Port 1 Constant Masks  
 unsigned char P1MDIN\_LO = 0xFD; // 1111 1101, Set P1.1 as an analog input   
 unsigned char P1MDOUT\_LO = 0xFD; // 1111 1101, Set P1.1 as a input port bit  
 unsigned char P1\_HI = 0x02; // 0000 0010 Set P1.1 to a high impedance state  
  
 // Port 2 Constant Masks  
 unsigned char P2MDOUT\_LO = 0xF0; // 1111 0000  
 unsigned char P2\_HI = 0x0F; // 0000 1111  
   
 // Port 3 Constant Masks  
 unsigned char P3MDOUT\_HI = 0xFC; // 1111 1100  
  
 // Set Port 1 analog input bits  
 P1MDIN &= P1MDIN\_LO;  
 // Set Port 1 output (low) bits  
 P1MDOUT &= P1MDOUT\_LO;  
 // Set Port 1 impedence (high) bits  
 P1 |= P1\_HI;  
  
 // Set Port 2 MDOUT low bits  
 P2MDOUT &= P2MDOUT\_LO;  
 // Set Port 2 impedence (high) bits  
 P2 |= P2\_HI;  
   
 // Set Port 3 MDOUT high bits  
 P3MDOUT |= P3MDOUT\_HI;  
}  
  
void Interrupt\_Init(void) {  
 // Enable Timer 0 Overflow interrupts (bit 1), and enable all interrupts (bit 7)  
 IE |= 0x82; // 1000 0010  
}  
  
//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  
void Timer\_Init(void) {  
 CKCON |= 0x08; // 0000 1000 (use SYSCLK)  
 TMOD &= 0xF0; // clear the 4 least significant bits (1111 0000)  
 TMOD |= 0x01; // 0000 0001 (Timer0 in mode 1, for 16-bit)  
 TR0 = 0; // Stop Timer0  
 TL0 = 0; // Clear low byte of register T0  
 TH0 = 0; // Clear high byte of register T0  
}  
  
void ADC\_Init(void) {  
 REF0CN &= 0xF7; // 1111 0111 Configure ADC1 to use VREF  
 REF0CN |= 0x03; // 0000 0011  
 ADC1CF = 0x01; // 0000 0001 Set a gain of 1  
 ADC1CN |= 0x80; // 1000 0000 Enable ADC1  
}  
  
unsigned char Read\_Port\_1(void) {  
 AMX1SL = 0x01; // 0000 0001 Set the Port pin number  
 ADC1CN &= 0xDF; // 1101 1111 Clear the flag from the previous ADC1 conversion  
 ADC1CN |= 0x10; // 0001 0000 Start A/D Conversion  
 while ((ADC1CN & 0x20) == 0x00); // Wait for conversion to be complete  
 return ADC1; //Assign the A/D conversion result  
}  
  
//\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*  
void Timer0\_ISR(void) interrupt 1 {  
 TF0 = 0; // clear interrupt request  
 Counts++;  
}  
  
/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/  
  
/\*  
\* Play the LITEC Memory game.  Returns if PB4 is ever pressed.  
\*/  
void play\_game(void) {  
 unsigned char turns[5], inputs[5], port1\_result, i, correct;  
 unsigned short on\_max\_counts, off\_max\_counts;  
  
 // Turn off all outputs  
 LED0 = 1;  
 LED1 = 1;  
 LED2 = 1;  
 BUZZER = 1;  
 BILED0 = 1;  
 BILED1 = 1;  
  
 // Calculate the on\_time and off\_time by reading Port 1’s A/D conversion  
 port1\_result = Read\_Port\_1();  
 on\_max\_counts = CalculateMaxCounts(port1\_result);  
 off\_max\_counts = (on\_max\_counts / 2);  
  
 // Generate the sequence of LEDs to light  
 turns[0] = unique\_random(3);  
 for (i = 1; i < 5; i++) {  
   // Generate a value different from the previous turn’s value.  
   turns[i] = unique\_random(turns[i - 1]);  
 }  
  
 // Light LED sequence  
 for (i = 0; i < 5; i++) {  
   // Restart the game if the player presses PushButton4.  
   if (light\_LED(turns[i], on\_max\_counts, off\_max\_counts) == 1) {  
     return;  
   }  
 }  
  
 // Light the green BiLED to indicate the ready-for-input state.  
 light\_green();  
  
 correct = 1;  
  
 for (i = 0; i < 5; i++) {  
   // Read a pushbutton, and record which one was pressed.  
   inputs[i] = ReadPushbuttons();  
   if (inputs[i] == 3) { // Pushbutton 4 pressed, restart game  
     return;  
   } else if (inputs[i] != turns[i]) { // Incorrect response  
     correct = 0;  
     printf("Input %d was incorrect!%s", i + 1, newline());  
     break;  
   } else { // Correct response  
     printf("Input %d was correct!%s", i + 1, newline());  
   }  
 }  
  
 if (correct) {  
   // flash LEDs 3 times  
   for (i = 0; i < 3; i++) {  
     // Turn LEDs on  
     LED0 = 0;  
     LED1 = 0;  
     LED2 = 0;  
     // Wait about a quarter of a second  
     Counts = 0;  
     while (Counts < 75);  
     // Turn LEDs off  
     LED0 = 1;  
     LED1 = 1;  
     LED2 = 1;  
     // Wait about a quarter of a second  
     Counts = 0;  
     while (Counts < 75);  
   }  
 } else {  
   // sounds buzzer for 1.5 seconds  
   BUZZER = 0;  
   light\_red();  
   Counts = 0;  
   while (Counts < 506);  
   BUZZER = 1; // Turn buzzer back off (thank God)  
 }  
  
 // Turn off BILED  
 BILED0 = 1;  
 BILED1 = 1;  
  
 // Wait for the Start Game button to be pressed  
 while (!CheckPushButton4());  
}  
  
/\*  
\* Returns the number of overflows to wait for in on\_time.  
\*  
\* NOTE: off\_time is simply (on\_time / 2).  
\*/  
int CalculateMaxCounts(unsigned char x) {  
 int on\_time\_millis = (x \* 5) + 200;  
 // This gives us the milliseconds to wait for.  In 16 bit counting mode,  
 // based on SYSCLK, there are exactly 337.5 overflows per second, or  
 // 0.3375 overflows per millisecond.  We multiply by this constant  
 // to convert from milliseconds to overflows.  
 return (on\_time\_millis \* 0.3375);  
}  
  
/\*  
\* Light the LED for on\_time, then wait for off\_time.  Returns 0 if successful, or 1  
\* if PushButton4 was pressed.  
\*/  
unsigned char light\_LED(unsigned char LED\_to\_light, short on\_time, short off\_time) {  
 switch(LED\_to\_light) {  
   case 0:  
     // Light LED0  
     LED0 = 0;  
     break;  
   case 1:  
     // Light LED1  
     LED1 = 0;  
     break;  
   case 2:  
     // Light LED2  
     LED2 = 0;  
     break;  
   default:  
     printf("Invalid LED input: %d%s", LED\_to\_light, newline());  
 }  
  
 // Wait for on\_time  
 Counts = 0;  
 while (Counts < on\_time) {  
   if (CheckPushButton4()) {  
     return 1;  
   }  
 }  
  
 // Turn LEDs off again  
 LED0 = 1;  
 LED1 = 1;  
 LED2 = 1;  
  
 // Wait for off\_time  
 Counts = 0;  
 while (Counts < off\_time) {  
   if (CheckPushButton4()) {  
     return 1;  
   }  
 }  
  
 return 0; // Pushbutton 4 not pressed  
}  
  
/\*  
\* Waits for a pushbutton to be pressed, then returns which button was pressed  
\* (as an integer between 0 and 3).  
\*/  
unsigned char ReadPushbuttons() {  
 while (1) {  
   if (CheckPushButton1()) {  
     Counts = 0;  
     while (Counts < 25); // Wait for PushButton to be completely pressed.  
     if (CheckPushButton1()) { // Check again, to make sure it was no accident  
       while (CheckPushButton1()); // Wait until the button is released.  
       Counts = 0;  
       while (Counts < 25); // Wait for PushButton to be completely released.  
       return 0;  
     }  
   }  
   if (CheckPushButton2()) {  
     Counts = 0;  
     while (Counts < 25); // Wait for PushButton to be completely pressed.  
     if (CheckPushButton2()) { // Check again, to make sure it was no accident  
       while (CheckPushButton2()); // Wait until the button is released.  
       Counts = 0;  
       while (Counts < 25); // Wait for PushButton to be completely released.  
       return 1;  
     }  
   }  
   if (CheckPushButton3()) {  
     Counts = 0;  
     while (Counts < 25); // Wait for PushButton to be completely pressed.  
     if (CheckPushButton3()) { // Check again, to make sure it was no accident  
       while (CheckPushButton3()); // Wait until the button is released.  
       Counts = 0;  
       while (Counts < 25); // Wait for PushButton to be completely released.  
       return 2;  
     }  
   }  
   if (CheckPushButton4()) {  
     Counts = 0;  
     while (Counts < 25); // Wait for PushButton to be completely pressed.  
     if (CheckPushButton4()) { // Check again, to make sure it was no accident  
       while (CheckPushButton4()); // Wait until the button is released.  
       Counts = 0;  
       while (Counts < 25); // Wait for PushButton to be completely released.  
       return 3;  
     }  
   }  
 }  
}  
  
/\*  
\* Returns a random number different from last\_state.  
\*/  
unsigned char unique\_random(unsigned char last\_state) {  
 unsigned char return\_value;  
 do {  
   return\_value = random(3);  
 } while(return\_value == last\_state);  
 return return\_value;  
}  
  
/\*  
\* Returns a random integer between 0 and N-1 (a range of N numbers).  
\*/  
unsigned char random(unsigned char N) {  
 return (rand() % N);  
}  
  
/\*  
\* Light BiLED green.  
\*/  
void light\_green(void) {  
 BILED0 = 0;  
 BILED1 = 1;  
}  
  
/\*  
\* :Light BiLED red.  
\*/  
void light\_red(void) {  
 BILED0 = 1;  
 BILED1 = 0;  
}  
  
/\*  
\* Returns a 0 if CheckPushButton1 not activated or a 1 if CheckPushButton1 is activated.  
\* This code reads a single input only, associated with PB1  
\*/  
int CheckPushButton1(void) {  
 // If PB1 is pressed, the value of PB1 is 0 (logic low).  If PB1 is not pressed, the  
 // value of PB1 is 1 (logic high).  This is the opposite of what makes sense in the  
 // code (with 0 usually meaning off, and 1 meaning on), so we negate the value in  
 // PB1 before returning.  
 return !PB1;  
}  
  
/\*  
\* Returns a 0 if push button 2 not activated or a 1 if push button 2 is activated.  
\* This code reads a single input only, associated with PB2  
\*/  
int CheckPushButton2(void) {  
 // If PB2 is pressed, the value of PB2 is 0 (logic low).  If PB2 is not pressed, the  
 // value of PB2 is 1 (logic high).  This is the opposite of what makes sense in the  
 // code (with 0 usually meaning off, and 1 meaning on), so we negate the value in  
 // PB2 before returning.  
 return !PB2;  
}  
  
/\*  
\* Returns a 0 if push button 3 not activated or a 1 if push button 3 is activated.  
\* This code reads a single input only, associated with PB3  
\*/  
int CheckPushButton3(void) {  
 // If PB3 is pressed, the value of PB3 is 0 (logic low).  If PB3 is not pressed, the  
 // value of PB3 is 1 (logic high).  This is the opposite of what makes sense in the  
 // code (with 0 usually meaning off, and 1 meaning on), so we negate the value in  
 // PB3 before returning.  
 return !PB3;  
}  
  
/\*  
\* Returns a 0 if push button 4 not activated or a 1 if push button 4 is activated.  
\* This code reads a single input only, associated with PB4  
\*/  
int CheckPushButton4(void) {  
 // If PB4 is pressed, the value of PB4 is 0 (logic low).  If PB4 is not pressed, the  
 // value of PB4 is 1 (logic high).  This is the opposite of what makes sense in the  
 // code (with 0 usually meaning off, and 1 meaning on), so we negate the value in  
 // PB4 before returning.  
 return !PB4;  
}  
  
/\*  
\* Helper function to return a string containing a newline character and return  
\* character.  
\*/  
char\* newline() {  
 char\* retval = "\r\n";  
 return retval;  
}

* 1. Hardware schematic




Figure 5b-1 – Lab 2 Hardware Schematic

## Participation Summary

MDS – Michael Stark

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Signature)

DMV – David Melecio-Vázquez

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

(Signature)

* Cover Sheet
  + Written: MDS
* Table of Contents
  + Written: MDS
* Introduction and Statement of Purpose
  + Written: DMV
* System Development
  + Written: MDS
  + Hardware Details
    - Written: MDS
    - Images: DMV
  + Software Details
    - Written:
    - Flowchart:
* Results and Conclusions
  + Written:
* Appendices
  + C Code
    - Included: MDS
  + Hardware Schematic
    - Designed in PSpice: MDS
  + Participation Summary
    - Written: MDS